***1.8 BIT ADDITION***

LDA 8500

MOV B,A

LDA 8501

ADD B

STA 8502

HLT

