***2.8 BIT SUBTRACTION***

LDA 9001

MOV B,A

LDA 9000

SUB B

STA 9002

HLT

